|  |  |  |
| --- | --- | --- |
|  |  | **INF.14** |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Ninety-ninth session 5 November 2015**

Geneva, 9 – 13 November 2015

Item 5 of the provisional agenda

**Work of the RID/ADR/ADN Joint Meeting**

Reference to standard EN 13094

Transmitted by the Government of France

Introduction

1. Referring to INF.9, it is proposed to amend the Table of 6.8.2.6.1 under “For design and construction of tanks” to add the reference of the new version of standard EN 13094 which was published in May **2015**.

2. As a consequence, for EN 13094:2008 + AC:2008, it is proposed to modify the text in Column (4) to read “Between 1 January 2011 and 31 December 2018”. This modification was adopted in March 2015 in the Standards Working Group (see INF.49) where the date “1 January 2011” was defined probably because the reference of this standard has appeared in the published version of RID/ADR 2011, while in documents INF.48 and INF.28 the date “1 January 2010” appears.

3. In October 2008, WP.15 adopted some amendments for entry into force on 1 July 2009 (see ECE/TRANS/WP.15/199, Annex I) including a reference to EN 13094:2008 to be applied as from 1 January **2010**.

Proposal

4. In 6.8.2.6.1, Amend the Table under "*For design and construction of tanks*" as follows:

For standard "EN 13094:2008 + AC:2008", in column (4), replace "Until further notice" by "Between 1 January **2010** and 31 December 2018".

After the standard "EN 13094:2008 + AC:2008", insert the following new standard:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| (1) | (2) | (3) | (4) | (5) |
| EN 13094:**2015** | Tanks for the transport of dangerous goods – Metallic tanks with a working pressure not exceeding 0.5 bar – Design and construction | 6.8.2.1 | Until further notice |  |