|  |  |  |
| --- | --- | --- |
|  |  | **INF.10**  |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**101st session 26 October 2016**

Geneva, 8–11 November 2016

Item 5(b) of the provisional agenda

**Proposals for amendments to annexes A and B of ADR:**

**miscellaneous proposals**

 Re-insert the heading for sub-section 7.5.5.3

 Transmitted by the Government of Sweden

 Introduction

The heading of sub-section 7.5.5.3 seems to have been deleted by mistake during the work with ADR 2009.

When reading the background documents related to the amendments proposed for sub-section 7.5.5.3, it seems there was no intention to delete the heading. The original proposal in [ECE/TRANS/WP.15/2006/12](http://www.unece.org/fileadmin/DAM/trans/doc/2006/wp15/ECE-TRANS-WP15-2006-12e.pdf) contained two options. The first option was to delete the entire sub-section 7.5.5.3, and the second option offered an alternative solution, which amended the text but remained the heading unchanged.

According to the report, ECE/TRANS/WP.15/190, the second option was adopted, where paragraph 17 reads as follows:

*“17. Following a vote, the Working Party rejected the proposal to delete 7.5.5.3 but adopted the proposal to increase the limits to 20 tonnes per transport unit (see annex 1).”*

However, in Annex 1 to the report, the heading was left out when the actual amendment was presented:

*“7.5.5.3 Amend to read as follows:*

*“7.5.5.3 The maximum quantity of organic peroxides of Class 5.2 and self-reactive substances of Class 4.1 of Types B, C, D, E or F is limited to20,000 kg per transport unit.”.”*

 Proposal

It seems that since the heading for sub-section 7.5.5.3 was left out in the report, it was not included in ADR 2009 or in the versions thereafter. We therefore propose to re-insert the heading of sub-section 7.5.5.3 as follows (underlined):

**“7.5.5.3 Limitations with respect to organic peroxides, self-reactive substances and polymerizing substances**

The maximum quantity of organic peroxides of Class 5.2 and self-reactive substances of Class 4.1 of Types B, C, D, E or F and of polymerizing substances of Class 4.1 is limited to 20 000 kg per transport unit.“