|  |  |  |
| --- | --- | --- |
|  |  | **INF.60** |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Joint Meeting of the RID Committee of Experts and the**

**Working Party on the Transport of Dangerous Goods 16 March 2016**

Bern, 14–18 March 2016

Item 6 of the provisional agenda

**Reports of informal working groups**

 Comments on document ECE/TRANS/WP.15/AC.1/2016/16 and INF 52

 Transmitted by the government of France

Special provision and Note:

Add a new special provision XXX in Chapter 3.3:

"XXX A trailer fitted with equipment, powered by a liquid or gaseous fuel or a battery, that is intended for use during a carriage operated by this trailer as a part of a transport unit, shall be subject to the same conditions as specified for vehicles assigned to UN 3166 or 3171, when carried as a load on a vehicle/wagon/vessel. Provided that the total capacity of the tanks containing liquid fuel does not exceed 500 litres."

NOTE to 1.1.3.2 a) and 1.1.3.3

"**Note:** A container fitted with equipment for use during carriage, fixed on a vehicle, is considered as an integral part of the vehicle and benefits from the same exemptions as regards to the fuel necessary to operate the equipment."

\_\_\_\_\_\_\_\_\_\_