|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.15/AC.2/2016/24 | |
| _unlogo | **Economic and Social Council** | | Distr.: General  3 November 2015  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Joint Meeting of Experts on the Regulations annexed to the  
European Agreement concerning the International Carriage  
of Dangerous Goods by Inland Waterways (ADN)  
(ADN Safety Committee)**

**Twenty-eighth session**

Geneva, 25–29 January 2016

Item 5 (b) of the provisional agenda

**Proposals for amendments to the Regulations annexed to ADN:**

**Other proposals**

Proposal to amend 7.2.4.25.5

Transmitted by the Governments of the Netherlands and France[[1]](#footnote-1)

|  |  |
| --- | --- |
| *Summary* |  |
| **Executive summary:** | Follow-up on the initial proposals made during the August 2015 ADN Safety Committee meeting |
| **Action to be taken:** | See paragraph 6. |
| **Related documents:** | ECE/TRANS/WP.15/AC.2/2015/18, ECE/TRANS/WP.15/AC.2/56, paras. 16 and 17 |

Introduction

1. At the 27th session of the ADN Safety Committee (August 2015), the Netherlands submitted for consideration document ECE/TRANS/WP.15/AC.2/2015/18, which contained a national (Dutch) interpretation relating to 7.2.4.25.5.

2. The Dutch proposal intended to also apply the provisions of the current 7.2.4.25.5 in the case where the previous cargo also required a "closed type vessel" according to column (7) of Table C of Chapter 3.2.

3. In its report ECE/TRANS/WP.15/AC.2/56, paras. 16 and 17, the Committee asked the Netherlands and France to submit a proposal for an amendment to 7.2.4.25.5 of the Regulations annexed to ADN.

4. As an additional remark, it is to be noted that column (7) of Table C of Chapter 3.2 deals with cargo tank design and does not deal with vessels, and that the wording “closed type vessel” is incorrectly used.

Proposed amendments

5. The proposed amendments takes into account the remark in paragraph 4 above, and the Dutch proposal contained in document ECE/TRANS/WP.15/AC.2/2015/18 (deleted text is struck through, **additional text is in bold underlined**):

"7.2.4.25.5 The gas/air mixtures shall be returned ashore through a vapour return piping during loading operations when:

* a closed ~~type vessel~~ **cargo tank** is required according to column (7) of Table C of Chapter 3.2;

**or**

* **a closed cargo tank according to column (7) of Table C of Chapter 3.2 was required for the previous cargo and the cargo tank is not gas free after unloading the previous cargo.**"

Follow-up

6. The Safety Committee is invited to consider the proposals in paragraph 5 above, and to take action as it deems appropriate.

1. Distributed in German by the Central Commission for the Navigation of the Rhine under the symbol CCNR-ZKR/ADN/WP.15/AC.2/2016/24. [↑](#footnote-ref-1)