|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2016/19 |
| Description: _unlogo | **Economic and Social Council** | Distr.: General23 December 2015Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**168th session**

Geneva, 8-11 March 2016

Item 4.9.4 of the provisional agenda

**1958 Agreement – Consideration of draft amendments**

**to existing Regulations submitted by GRE**

Proposal for Supplement 9 to the 05 series of amendments to Regulation No. 48 (Installation of lighting and light-signalling devices)

**Submitted by the Working Party on Lighting and Light-Signalling**[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on Lighting and Light-Signalling (GRE) at its seventy-fourth session (ECE/TRANS/WP.29/GRE/74, paras. 15 and 17). It is based on ECE/TRANS/WP.29/GRE/2015/21 and Annex II to the report. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee AC.1 for consideration at their March 2016 sessions.

*Paragraph 6.2.9.*, amend to read:

"6.2.9. Other requirements

The requirements of paragraph 5.5.2. shall not apply to dipped-beam headlamps.

Dipped-beam headlamps with a light source or LED module( s) producing the principal dipped beam and having a total objective luminous flux which exceeds 2,000 lumens shall only be installed in conjunction with the installation of headlamp cleaning device( s) according to Regulation No. 45.11

With respect to vertical inclination the provisions of paragraph 6.2.6.2.2. above shall not be applied for dipped-beam headlamps with a light source or LED module(s) producing the principal dipped beam and having an objective luminous flux which exceeds 2,000 lumens.

In the case of filament lamps for which more than one test voltage is specified, the objective luminous flux which produces the principal dipped beam, as indicated in the communication form for the type approval of the device, is applied.

…"

*Paragraph 6.13.2.*,amend to read:

"6.13.2. Number

 Two visible from the front and two visible from the rear.

 Additional lamps may be fitted as follows:

 (a) Two visible from the front;

 (b) Two visible from the rear."

*Paragraph 6.13.4.2., last indent*, amend to read:

"6.13.4.2. …

 The additional lamps, as specified in paragraph 6.13.2. (b), shall be fitted as far separated in height as practicable in respect to the mandatory ones, provided that their position is compatible with design/operational requirements of the vehicle and symmetry of the lamps."

*Paragraph 6.13.4.3.*,amend to read:

"6.13.4.3. In length, no special requirement.

 The additional lamps, as specified in paragraph 6.13.2. (a), shall be fitted as close as practicable to the rear; this requirement shall be deemed to be satisfied if the distance between the additional lamps and the rear of the vehicle does not exceed 400 mm."

*Paragraph 6.13.9.*, *after the last indent, add a new indent* to read:

"6.13.9. …

 The additional lamps, as specified in paragraph 6.13.2. (a), used to mark the rear end outline of the vehicle, the trailer or the semi-trailer shall be fitted in such a way to make it visible within the fields of vision of the approved main rear-view devices for indirect vision."

1. \* In accordance with the programme of work of the Inland Transport Committee for 2014–2018 (ECE/TRANS/240, para. 105 and ECE/TRANS/2014/26, programme activity 02.4), the World Forum will develop, harmonize and update Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)