|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2017/76 |
| Description: _unlogo | **Economic and Social Council** | Distr.: General10 April 2017Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**172nd session**

Geneva, 20-23 June 2017

Item 4.10.5 of the provisional agenda

**1958 Agreement: Consideration of draft amendments**

**to existing Regulations submitted by GRE**

Proposal for Supplement 10 to the 04 series of amendments to Regulation No. 19 (Front fog lamps)

**Submitted by the Working Party on Lighting and Light-Signalling**[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on Lighting and Light-Signalling (GRE) at its seventy-seventh session (ECE/TRANS/WP.29/GRE/77). It is based on ECE/TRANS/WP.29/GRE/2017/7 and Annex IV to ECE/TRANS/WP.29/GRE/77. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee AC.1 for consideration at their June 2017 sessions.

Supplement 10 to the 04 series of amendments to Regulation No. 19 (Front fog lamps)

*Paragraph 5.6.,* amend to read:

"5.6. In the case of Class B, the front fog lamp shall onlybe equipped with one filament light source approved according to Regulation No. 37, even if the filament light source cannot be replaced. Any Regulation No. 37 approved filament light source may be usedprovidedthat;

(a) Its objective luminous flux does not exceed 2,000 lumens, and

(b) No restriction on the use is made in Regulation No. 37 and its series of amendments in force at the time of application for type approval.

5.6.1. Even if this filament light source cannot be replaced it shall comply with the requirements in paragraph 5.6. above."

*Paragraph 5.7.,* amend to read:

"5.7*.* In the case of Class F3, irrespective of whether the light sources can be replaced or not, the front fog lamp shall only be equipped with:

5.7.1. One or more light sources approved according to:

5.7.1.1. Regulation No. 37 and its series of amendments in force at the time of application for type approval, provided that no restriction on their use is made,

5.7.1.2. Or, Regulation No. 99 and its series of amendments in force at the time of application for type approval,

5.7.2. And/or, one or more LED modules where the requirements of Annex 12 to this Regulation shall apply; compliance with these requirements shall be tested."

1. \* In accordance with the programme of work of the Inland Transport Committee for 2016–2017 (ECE/TRANS/254, para. 159 and ECE/TRANS/2016/28/Add.1, cluster 3.1), the World Forum will develop, harmonize and update Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)