|  |  |
| --- | --- |
| Submitted by the experts from CLEPA and  The European Commission | Informal document **GRRF-83-31**  83rd GRRF, 23-27 January 2017  Agenda item 3(c) |

Proposal for amendments to Footnote 12 in Regulation No. 13

*Footnote 12*, amend to read:

"12 Off-road vehicles, special purpose vehicles (e.g. mobile plant using nonstandard vehicle chassis, mobile cranes, hydro-static driven vehicles in which the hydraulic drive system is also used for braking and auxiliary functions, **vehicles having a non-standard chassis where the installation of sensor(s) for values of lateral acceleration and/or yaw rate, necessary for the function of the stability control, cannot be installed within the specified area close to the center of gravity of the vehicle without compromising its special purpose),** N2 vehicles which have all of the following features: a gross vehicle mass between 3.5 and 7.5 tonnes, a non-standard low-frame chassis, more than two axles and hydraulic transmission, Class I and Class A buses of categories M2 and M3, articulated buses and coaches, N2 tractors for semi-trailer with a gross vehicle mass (GVM) between 3.5 and 7.5 tonnes shall be excluded from this requirement."

.