|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2018/123 | |
| Description: _unlogo | **Economic and Social Council** | | Distr.: General  15 August 2018  English  Original: English and French |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**176th session**

Geneva, 13-16 November 2018

Item 4.7.4 of the provisional agenda

**1958 Agreement:  
Consideration of draft amendments**

**to existing UN Regulations submitted by GRSG**

Proposal for Supplement 6 to the 04 series of amendments to UN Regulation No. 46 (Devices for indirect vision)

**Submitted by the Working Party on General Safety Provisions**[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on General Safety Provisions (GRSG) at its 114thsession (ECE/TRANS/WP.29/GRSG/93, para. 19). It is based on official document ECE/TRANS/WP.29/GRSG/2018/9 as reproduced in paragraph 19 to the report. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee AC.1 for consideration at their November 2018 sessions.

Supplement 6 to the 04 series of amendments to UN Regulation No. 46 (Devices for indirect vision)

*Paragraph 16.1.1.3.,* amend to read:

"16.1.1.3. Overlay requirements within the minimum required field of vision

Overlays shall display only safety-related rearward vision information.

All overlays shall …… worst case(s)."

*Annex 3*

*Item 9,* amend to read (replacing the letter "S" by class "VII" and keeping the reference to footnote 2 unchanged):

"9. Brief description

Identification of the device: mirror, camera/monitor, other devices for indirect vision of Classes I, II, III, IV, V, VI, VII 2

Symbol ……"

1. \* In accordance with the programme of work of the Inland Transport Committee for 2018–2019 (ECE/TRANS/274, para. 123 and ECE/TRANS/2018/21/Add.1, Cluster 3.1), the World Forum will develop, harmonize and update UN regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)