|  |  |
| --- | --- |
| Transmitted by the expert from SAE | Informal document **GRE-79-32-Rev.1**  (79th GRE, 24-27 April 2018,  agenda item 4)) |

**Proposal for a:**

**Supplement [x]to the [y] series of amendments of Regulation No. 98**

**Supplement [x]to the [y] series of amendments of Regulation No. 112**

**Supplement [x]to the [y] series of amendments of Regulation No. 113**

**Supplement [x]to the [y] series of amendments of Regulation No. 123**

Proposal to keep UN Regs 98, 112, 113 and 123 alive for the purpose of Canadian CMVSS 108:

**Proposal:**

UN Reg. 98

*Add new paragraph 5.14., to read:*

5.14. Irrespective of the requirements in paragraph 5., 6. and 7., lamps satisfying requirements of the latest version of UN Regulation [RID] as it relates to headlamps equipped with gas-discharge light sources shall be deemed complying with this UN Regulation.

Alternatively:

5.14 Instead of requirements of this UN Regulation, headlamps may conform with requirements of the latest version of the UN Regulation [RID] as it relates to headlamps equipped with gas-discharge light sources.”

UN Reg. 112

*Add new paragraph 5.12., to read:*

5.12. Irrespective of the requirements in paragraph 5., 6., 7. and 8., lamps satisfying requirements of the latest version of UN Regulation [RID] as it relates to headlamps emitting an asymmetric passing beam shall be deemed complying with this UN Regulation.

Alternatively:

5.12 Instead of requirements of this UN Regulation, headlamps may conform with requirements of the latest version of the UN Regulation [RID] as it relates to headlamps emitting an asymmetric passing beam.

UN Reg. 113

*Add new paragraph 5.11., to read:*

5.11. Irrespective of the requirements in paragraph 5., 6., and 7., lamps satisfying requirements of the latest version of UN Regulation [RID] as it relates to headlamps emitting a symmetric passing beam shall be deemed complying with this UN Regulation.

Alternatively:

5.11. Instead of requirements of this UN Regulation, headlamps may conform with requirements of the latest version of the UN Regulation [RID] as it relates to headlamps emitting a symmetric passing beam.

UN Reg. 123

*Add new paragraph 5.16., to read:*

5.16. Irrespective of the requirements in paragraph 5., 6., and 7., lamps satisfying requirements of the latest version of UN Regulation [RID] as it relates to the adaptive forward-illumination system shall be deemed complying with this UN Regulation.

Alternatively:

5.16. Instead of requirements of this UN Regulation, headlamps may conform with requirements of the latest version of the UN Regulation [RID] as it relates to the adaptive forward-illumination system.

**Justification:**

Recent amendment to Canada Motor Vehicle Safety Standards (CMVSS) 108 allows UN Regulation headlamp to be used on vehicles in Canada. CMVSS 108 specifically refers to present UN Regulations. These Regulations are to be soon frozen and no more improvements will be added to them.

To continue in Canada the allowance of the UN Reg headlamps conforming to the new UN Reg [RID] the frozen UN Regulations should make a clear reference to UN Reg [RID].