|  |  |
| --- | --- |
| Submitted by the experts from ETRTO | Informal document **GRRF-86-26**  86th GRRF, 12-16 February 2018  Agenda item 7(c) |

Proposal for amendments to   
ECE/TRANS/WP.29/GRRF/2018/5 and ECE/TRANS/WP.29/GRRF/2018/11

I. Proposal

*Annex 5, Part II, Table B, Column header* amend to read:

"

| *Tyre-size designation1****,4*** | *Measuring rim width code* | *Nominal rim diameter*  *d (mm)* | *Outer diameter D (mm)2* | | *Section width S (mm)3* |
| --- | --- | --- | --- | --- | --- |
| ***Highway Tread6*** | ***Traction Tread5*** |
| … | … | … | … | … | … |

"

*Annex 5, Part II, Table B, footnote 2,* amend to read:

"2 Coefficient 'b' for the calculation of Dmax: 1.07. **The manufacturer shall declare in section 9 of the communication form in Annex 1 (‘Any remarks’) the type of tread selected for the application.**"

*Annex 5, Part II, Table B, footnote 5,* amend to read:

"**5  Traction tread tyres are those bearing at least one of the following inscriptions:**

**- Inscription(s) defined in section 3.1.12. of this Regulation.**

**- Alpine symbol (3PMSF) as defined in UN Regulation 117.**

**- “TRACTION” inscription as defined in UN Regulation 117.**"

*Annex 5, Part II, Table B, footnote 6* amend to read:

"**6 Highway tread tyres are all tyres that are not Traction tread.**"

II. Justification

It is proposed to amend a footnote in Annex 5 to avoid misunderstandings with the definition of “category of use”.