##### INF. 16/Rev.1

27 September2019

Original: German

**RID/ADR/ADN**

Joint Meeting of the RID Committee of Experts and the

Working Party on the Transport of Dangerous Goods

(Geneva, 17 - 27 September 2019)

**Item 7 of the agenda: Reports of informal working groups**

**Chapter 6.2 – Consequential amendments concerning the proposals made by the informal working group on the inspection and certification of tanks**

**Submitted by Germany on behalf of the Working Group on Tanks**

***Note:*** *This document contains the text as agreed by the Working Group on Tanks. The representative of Germany added a few editorial comments for further consideration.*

**Introduction**

1. The informal working group on the inspection and certification of tanks met from 12 to 14 June 2019 and again from 10 to 11 July 2019 and has submitted amendments to sections 1.8.6 and 1.8.7 in conjunction with Chapter 6.8 (see informal document INF.19).

2. The proposed amendments to sections 1.8.6 and 1.8.7 also have an impact on Chapter 6.2, as this chapter draws on the provisions of sections 1.8.6 and 1.8.7. Thus, amendments to Chapter 6.2 are also necessary.

3. These consequential amendments to Chapter 6.2 go beyond the amendments that only concern tanks. Therefore, Germany has agreed to submit these amendments in a separate document.

4. INF 16/Rev.1 details the changes to align the text with the conclusions of the Informal working goup and Working Group on Tanks.

**Proposals**

5. Germany thus proposes that Chapter 6.2 be amended as follows:

**6.2.2.11** Make the following amendments to the table:

– After “Type approval (1.8.7.2)”, insert a reference to a footnote which reads as follows:

"\* When an inspection body is designated by the competent authority to issue the type approval certificate, the type examination shall be performed by that inspection body.”

* Combine rows three and four in the table to read;

|  |  |
| --- | --- |
| Supervision of manufacture (1.8.7.3) and initial inspection and tests (1.8.7.4). | Xa or IS |

– In the last row amend “(1.8.7.5)” to read:

“(1.8.7.6)”.

* Add the following text after the table;

“Each procedure as defined in the table has to be performed by a single relevant body.”

Amend the first sub-paragraph after the table as follows:

– Delete:

“, its delegate”.

– Replace “conforming to 1.8.6.2, 1.8.6.4, 1.8.6.5 and 1.8.6.8” by:

“conforming to 1.8.6.3”.

In the second sub-paragraph after the table, replace “conforming to 1.8.6.2, 1.8.6.4, 1.8.6.5 and 1.8.6.8” by:

“conforming to 1.8.6.3”.

Amend the third sub-paragraph after the table as follows:

– Replace “the applicant” by:

“the manufacturer or the testing facility”.

– Replace “conforming to 1.8.6.2, 1.8.6.4, 1.8.6.5 and 1.8.6.8” by:

“conforming to 1.8.6.3”.

Add the following sub-paragraphs at the end:

“If an in-house inspection service has been used for the initial inspection and test , the mark specified in 6.2.2.7.2 (d) shall be accompanied by the mark of the in-house inspection service.

If an in-house inspection service has carried out the periodic inspection , the mark specified in 6.2.2.7.2 (b) shall be accompanied by the mark of the in-house inspection service.”

**6.2.3.6.1** In the first row of the table, replace “Type approval (1.8.7.2)” by:

“Type examination and type approval certificate issue (1.8.7.2)\*

\_\_\_\_\_

\* The type approval certificate shall be issued by the inspection body that performed the type examination.”

Combine rows three and four in the table to read;

|  |  |
| --- | --- |
| Supervision of manufacture (1.8.7.3) and initial inspection and tests (1.8.7.4). | Xa or IS |

Add the following text after the table;

“Each procedure as defined in the table has to be performed by a single relevant body.”

Amend the second sub-paragraph after the table as follows:

– Delete:

“, its delegate”.

– Replace “conforming to 1.8.6.2, 1.8.6.4, 1.8.6.5 and 1.8.6.8” by:

“conforming to 1.8.6.3”.

In the third sub-paragraph after the table, replace “conforming to 1.8.6.2, 1.8.6.4, 1.8.6.5 and 1.8.6.8” by:

“conforming to 1.8.6.3”.

Amend the forth sub-paragraph after the table as follows:

– Replace “the applicant” by:

“the manufacturer or the testing facility”.

– Replace “conforming to 1.8.6.2, 1.8.6.4, 1.8.6.5 and 1.8.6.8” by:

“conforming to 1.8.6.3”.

**6.2.3.8** Replace “1.8.6” by:

“1.8.6.3”

**6.2.3.9.3** Add the following sub-paragraph at the end:

“The requirements of 6.2.2.7.4 (n) shall be replaced by the following:

(n) the manufacturer’s mark. When the country of manufacture is not the same as the country of approval, then the manufacturer's mark shall be preceded by the character(s) identifying the country of manufacture as indicated by the distinguishing sign used on vehicles in international road traffic2). The country mark and the manufacturer’s mark shall be separated by a space or slash;”

\_\_\_\_\_\_\_\_\_\_