UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/746
8 December 2000

ENGLISH

Original: ENGLISH

and FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

World Forum for Harmonization of Vehicle Regulations (WP.29)

DRAFT SUPPLEMENT 11 TO THE 04 SERIES OF AMENDMENTS

TO REGULATION No. 16

(Safety-belts)

Note: The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its sixteenth session, following the recommendation by WP.29 at its one-hundred-and-twenty-second session. It is based on document TRANS/WP.29/2000/54, not amended (TRANS/WP.29/743, para. 147).

__________

Paragraph 6.4.1.3.2., amend to read:

"..... between 100 and 300 mm at chest level. In the case of a harness belt, the minimum displacements specified above may be reduced by half. These displacements are the displacements in relation ....."

__________

GE.00-