**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Joint Meeting of the RID Committee of Experts and the
Working Party on the Transport of Dangerous Goods 23 September 2021**

Geneva, 21 September – 1 October 2021
Item 2 of the provisional agenda

**Tanks**

 Corrigendum to ECE/TRANS/WP.15/AC.1/2021/23/Rev.1

 Supplementary information from the informal working group on the inspection and certification of tanks: Proposed amendments to Chapters 6.8 and 6.2, sections 1.8.7 and 1.8.6, plus transitional measures and consequential amendment

 Corrigendum

**1. Chapter 6.8**

*6.8.1.5.5: Amend the text to read:*

*“*To perform the entry into service verification, the owner or operator of the tank shall engage a single inspection body different to the inspection bodies engaged for the **~~original~~** type examination, supervision of manufacture or initial inspection. The inspection body …”

*6.8.3.4.13: Amend the text to read:*

### “6.8.3.4.13 In footnote 1**~~9~~8**/12, replace “the expert approved by the competent authority” by “the competent authority”.

1. **Chapter 1.8.7**

*1.8.7.1.5: Amend the text in the first paragraph to read:*

“ ~~Design t~~Type approval certificates, ~~and~~ inspection certificates ~~of conformity~~ and reports for the products (pressure receptacles, tanks, elements and structural and service equipment**,** **~~or~~** battery-wagons/battery-vehicles or MEGCs), including the technical documentation, shall be ~~retained~~ kept:”

*1.8.7.7.1: Amend the text to read:*

### 1.8.7.7~~6~~.1 ~~The applicant shall:~~ Where an in-house inspection service is used according to 6.2.2.1**~~1~~**2, 6.2.3.6.1**[, ~~or~~ 6.8.1.5.3 (b) or 6.8.1.5.4 (b)]**, the manufacturer or the testing facility shall:

(a) Implement ~~an in-house inspection service with~~ a quality system for the in-house inspection service, including technical procedures, for inspections and tests documented in 1.8.7.8~~7~~.6~~5~~ and subject to surveillance;

(b) Fulfil the obligations arising out of the quality system as approved and ~~to~~ ensure that it remains satisfactory and efficient in particular:

(i~~c~~) ~~Appoint~~ Authorize trained and competent personnel for the in-house inspection service; and

(ii~~d~~) Affix the ~~registered~~ identity mark or stamp, **as specified in Chapters 6.2 and 6.8,** of the inspection body, and the mark of the in-house inspection service where appropriate on the product to ensure traceability.

*1.8.7.2.2.2: Amend the text in the first paragraph to read:*

“The type approval shall be valid for a maximum of ten years. If within that period~~,~~ the relevant technical requirements of RID/ADR, ~~(~~including the referenced standards~~)~~, have changed so that the approved type is no longer in conformity with them, ~~the relevant body which issued~~ then the type approval is no longer valid. If within that period, the withdrawal date according to column (3) of the tables in 6.2.2.1 a**n**d 6.2.2.3 or column (5) of the tables in 6.2.4.1**,** **~~and~~** 6.8.2.6.1 **~~or~~ and** 6.8.3.6 applies the type approval is also no longer valid. …”

*1.8.7.2.2.2: Amend the second note to read:*

*NOTE: ~~In such a case, t~~The relevant provisions concerning the use, periodic inspection and intermediate inspection of products ~~pressure receptacles, tanks, battery-vehicles/battery-wagons or MEGCs~~ contained in a ~~the~~ type approval which has expired or has been withdrawn shall continue to apply to the~~se~~ products ~~pressure receptacles, tanks, battery-vehicles/battery-wagons or MEGCs~~ constructed according to that type approval before ~~the~~ its expiry or ~~the~~ its withdrawal if they may continue to be used.* ***~~They may continue to be used as long as they remain in conformity with the requirements of RID/ADR. If they are no longer in conformity with the requirements of RID/ADR they may continue to be used only if such use is permitted by relevant transitional measures in Chapter 1.6.~~***

*1.8.7.2.2.2: Amend the paragraph after second note to read:*

Type approvals may be renewed on the basis of ~~by a complete review and assessment~~ a new type examination ~~for conformity~~. Results of the previous type examination tests shall be taken into account if these tests are still in accordance with the provisions of RID/ADR **including the standards** applicable at the date of renewal. Renewal is not permitted after a type approval has been withdrawn.

*1.8.7.5.1: Amend the text to read:*

“If an entry into service verification is required by the competent authority under 6.8.1.5.5, the owner or operator shall engage a single inspection body to perform th**e~~is~~** **~~inspection~~** **entry into service verification** and shall provide it with the type approval certificate and the technical documentation specified in 1.8.7.8.4.”

1. **Chapter 1.8.6**

*Amend the Notes at the start of 1.8.6 to read:.*

### “**1.8.6 Administrative controls for the activities ~~application of the conformity assessments, periodic inspections, intermediate inspections and exceptional checks~~ described in 1.8.7 and 1.8.8**

**NOTE 1: For the purpose of this section the terms:**

**- "approved inspection body" means an inspection body approved by the competent authority to perform different activities according to 1.8.6.1, and**

**- "recognized inspection body" means an approved inspection body recognized by another competent authority.**

**NOTE 2: An inspection body may be designated by the competent authority to act as the competent authority (see the definition of competent authority in 1.2).**

*1.8.6 Note 2: Amend the Note to read:*

“NOTE 2: An inspection body may be designated by the competent authority to act as the competent authority (see the definition of competent authority in 1.2**.1**).”

*1.8.6.3.4: Amend the paragraph number to read:*

1.8.6.**~~5~~**~~.~~3.4*Information obligations ~~for inspection bodies~~*