**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Joint Meeting of the RID Committee of Experts and the
Working Party on the Transport of Dangerous Goods 30 September 2021**

Geneva, 21 September – 1 October 2021
Item 2 of the provisional agenda

**Tanks**

Comments on ECE/TRANS/WP.15/AC.1/2021/36

 Mandatory fitting of safety valves to tanks carrying flammable liquefied gases

 Transmitted by the Government of France

**Introduction**

The conditions of calculation and interpretation of the calculation are missing. They need to be introduced otherwise the text is not applicable.

**Proposals**

At the end of the new 6.8.3.2.9.1:

* Replace the reference to “6.7.3.8.1.1” by “6.7.3.8.1 and the safety valve shall conform at least to the requirement of 6.7.3.9.”
* And add the following Note:

“*NOTE : For the application of this paragraph, the value “120% of the MAWP” given in 6.7.3.8.1 shall be replaced by 0.9 times the test pressure of the tank*.”

A la fin du nouveau 6.8.3.2.9.1:

* Remplacer la référence au "6.7.3.8.1.1" par "6.7.3.8.1 et la soupape de sécurité doit être conforme au moins aux prescriptions du 6.7.3.9."
* Et ajoutez le Nota suivant:

« *NOTA : Pour l'application de ce paragraphe, la valeur de 120% de la PMSA indiquée au 6.7.3.8.1 doit être remplacée par 0,9 fois la pression d'épreuve de la citerne.* »