Corrections to ECE/TRANS/WP.29/2022/93

This proposal is based on ECE/TRANS/WP.29/GRE/2022/4 which was adopted by GRE at its 86th session in April 2022.

*Paragraph* 3.3.2.4.2*.,* for "by means of" read "with or without".

*Table 6, Part A,* *row* "*Segment 10 and below", last column,* for "50R" read "25V".

*Paragraph 5.2.3.,* amend to read:

“5.2.3. There shall be no lateral variations detrimental to good visibility in zone III.”

*Table 7, Part A,* *row "S100+S100LL+S100RR", third column,* for "3.75∙103 d " read "3.75∙102d ".

*Table 7, Part A,* *row* "*Segment 10 and below", seventh column,* for "50R" read "25V".

*Table 16, row "Segment 6", last column,* amend to read: "0.8 x the actual measured value at point 1.72°D-V".

*Annex 1, item 9.1.8.,* for "4.5.3.4." read "4.5.3.5."