|  |
| --- |
| **UN/SCETDG/61/INF.39** |
| **Committee of Experts on the Transport of Dangerous Goodsand on the Globally Harmonized System of Classificationand Labelling of Chemicals****Sub-Committee of Experts on the Transport of Dangerous Goods 22 November 2022****Sixty-first session**Geneva, 28 November-6 December 2022Item 2 (a) of the provisional agenda**Recommendations made by the Sub-Committee at its fifty-eighth, fifty-ninth and sixtieth sessions and pending issues:review of draft amendments already adopted during the biennium** |

 Corrections to document ST/SG/AC.10/C.3/2022/75

 Note by the secretariat

 I. Introduction

1. The secretariat suggests three corrections to document ST/SG/AC.10/C.3/2022/75.

 1. Editorial amendment to the new heading in 6.1.4.12

2. We believe that the amended heading in 6.1.4.12 would read better as “***Fibreboard boxes (including corrugated fibreboard boxes)***” instead of “***Fibreboard (including corrugated fibreboard) boxes***”. Proposal 1 contains the corrected amendment.

 Proposal 1

6.1.4.12 Amend the heading to read:

“**6.1.4.12 *Fibreboard boxes (including corrugated fibreboard boxes)***”.

 2. Mistake in 6.2.2.4

3. The objective of the last amendment to 6.2.2.4 was simply to change the notation with which an amendment to an ISO standard was referenced in the text, to bring it in line with other references. However, the amendment as adopted also changed the dates of the ISO standard and its amendment. We have with ISO confirmed that the changes in the dates were an unintended typo. Proposal 2 contains the corrected amendment.

 Proposal 2

6.2.2.4 In the first table, in the row for ISO 18119:2018, replace “Until further notice” by “Until 31 December 2026”. Add a new row beneath this row as follows:

|  |  |  |
| --- | --- | --- |
| ISO 18119:2018 +Amd 1:2021 | Gas cylinders – Seamless steel and seamless aluminium-alloy gas cylinders and tubes — Periodic inspection and testing | Until further notice |

 For ISO 10461:2005/A1:2006, replace “ISO 10461:2005/A1:2006” by “ISO 10461:2005 + Amd 1:2006”.

 3. Mistake in 6.2.2.11

4. The new note in 6.2.2.11 contains a spurious “constructed” which should be deleted. Proposal 3 contains the corrected amendment.

 Proposal 3

6.2.2.11 Insert the following note at the end:

“***NOTE:*** *Closures of refillable pressure receptacles manufactured before 1 January 2027 in accordance with the requirements applicable in the twenty-first revised edition of the Model Regulations which are not marked in accordance with the requirements of 6.2.2.11 applicable in the twenty-second revised edition may continue to be used.*”