|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/GRSP/2023/10 |
| _unlogo | **Economic and Social Council** | Distr.: General1 March 2023Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**Working Party on Passive Safety**

**Seventy-third session**

Geneva, 15–19 May 2023

Item 10 of the provisional agenda

**Regulation No. 100 (Electric power trained vehicles)**

 Proposal for the 04 Series of Amendments to Regulation No. 100 (Electric power trained vehicles) [[1]](#footnote-2)\*

 Submitted by the expert from the Netherlands

The text reproduced below was prepared by the expert from the Netherlands, aimed to an identification of buses and trucks equipped with an electric drivetrain which is consistent with existing regulated identification for Liquified Petroleum Gas (LPG), Compressed Natural Gas (CNG), Liquid Natural Gas (LNG) and Compressed Hydrogen (H2) fuelled trucks and busses. The modifications to the current text of the UN Regulation are marked in bold for new or strikethrough for deleted characters.

 I. Proposal

*Contents, list of annexes,* amend to read:

"Contents

 *Page*

Regulation

1. Scope

2. Definitions

3. Application for Approval

4. Approval

5. Part I: Requirements of a Vehicle with Regard to Specific Requirements for the Electric Power Train

6. Part II: Requirements of a Rechargeable Electrical Energy Storage System with Regard
to its Safety

7. Modifications and extension of the type approval

8. Conformity of production

9. Penalties for non-conformity of production

10. Production definitively discontinued

11. Names and addresses of Technical Services responsible for conducting approval tests and
of Type Approval Authorities

12. Transitional provisions

Annexes

1 Part 1 - Communication concerning the approval or extension or refusal or withdrawal of approval
or production definitively discontinued of a vehicle type with regard to its electrical safety pursuant
to Regulation No. 100

1 Part 2 - Communication concerning the approval or extension or refusal or withdrawal of approval
or production definitively discontinued of a REESS type as component/separate technical unit
pursuant to Regulation No. 100

1 Appendix 1

1 Appendix 2

2 Arrangements of the Approval Marks

3 Protection against direct contacts of parts under voltage

4 Verification of potential equalization

5A Isolation resistance measurement method for vehicle based tests

5B Isolation resistance measurement method for component based tests of a REESS

6 Confirmation method for function of on-board isolation resistance monitoring system

7A Verification method for testing authorities confirming document based isolation resistance
compliance of electrical design of the vehicle after water exposure

7B Vehicle-based test procedure for protection against water effects

8 Determination of hydrogen emissions during the charge procedures of the REESS

 Appendix 1 - Calibration of equipment for hydrogen emission testing

 Appendix 2 - Essential characteristics of the vehicle family

9 REESS test procedures

 Appendix 1 - Procedure for conducting a standard cycle

 Appendix 2 – Procedure for SOC adjustment

9A Vibration test

9B Thermal shock and cycling test

9C Mechanical shock

9D Mechanical integrity

9E Fire resistance

Appendix 1 - Dimension and technical data of firebricks

9F External short circuit protection

9G Overcharge protection

9H Over-discharge protection

9I Over-temperature protection

9J Over-current protection

**10 Provisions for a Label for Vehicles of Categories M2/N2 and M3/N3 Equipped with
an Electric Power Train "**

*Insert a new paragraph 5.5.,* to read:

**"5.5. Identification of electric power trained vehicles.**

**5.5.1. On vehicles of the categories M2/N2 and M3/N3, equipped with a high voltage electric powertrain, labels shall be installed as specified in Annex 10.**

**5.5.2. For hybrid electric vehicles running on diesel or gasoline, the high voltage powertrain shall be considered its first energy source, independent of the capacity of the REESS.**

**5.5.3. The labels shall be installed on the front and rear of the vehicle and on the outside of the doors on the right-hand side (left-hand drive vehicles) and left-hand side (right-hand drive vehicles)."**

*Paragraph 12.6.,* renumber as paragraph 12.10.

*Insert new paragraphs 12.6. to 12.9*., to read:

**"12.6. As from the official date of entry into force of the 04 series of amendments, no Contracting Party applying this UN Regulation shall refuse to grant or refuse to accept UN type approvals under this UN Regulation as amended by the 04 series of amendments.**

**12.7. As from 1 September 2025, Contracting Parties applying this UN Regulation shall not be obliged to accept UN type approvals to the preceding series of amendments that were first issued on or after 1 September 2025.**

**12.8. Until 1 September 2026, Contracting Parties applying this UN Regulation shall accept UN type approvals to the preceding series of amendments that were first issued before 1 September 2025.**

**12.9. As from 1 September 2026, Contracting Parties applying this Regulation shall not be obliged to accept type approvals issued to the preceding series."**

*Annex 2,* amend to read:

"Annex 2

 Arrangements of the Approval Marks

# Model A

# (See paragraph 4.4. of this Regulation)

# Figure 1

 a = 8 mm min.

**100 R - 042492**



The approval mark in Figure 1 affixed to a vehicle shows that the road vehicle type concerned has been approved in the Netherlands (E 4), pursuant to Regulation No. 100, and under the approval number **04**2492. The first two digits of the approval number indicate that the approval was granted in accordance with the requirements of Regulation No. 100 as amended by **04** series of amendments.

# Figure 2



**100 RES - 042492**



a = 8 mm min.

The approval mark in Figure 2 affixed to a REESS shows that the REESS type ("ES") concerned has been approved in the Netherlands (E 4), pursuant to Regulation No. 100, and under the approval number **04**2492. The first two digits of the approval number indicate that the approval was granted in accordance with the requirements of Regulation No. 100 as amended by **04** series of amendments.

# Model B

(See paragraph 4.5. of this Regulation)



|  |  |
| --- | --- |
| **100** | **04 2492** |
| **42** | **00 1628** |



a = 8 mm min.

The above approval mark affixed to a vehicle shows that the road vehicle concerned has been approved in the Netherlands (E4) pursuant to Regulations Nos. 100 and 42[[2]](#footnote-3). The approval number indicates that, at the dates when the respective approvals were granted, Regulation No. 100 was amended by the **04** series of amendments and Regulation No. 42 was still in its original form."

*Introduce a new Annex 10,* to read:

**"Annex 10**

 **Provisions for a Label for Vehicles of Categories M2/N2 and M3/N3 Equipped with an Electric Power Train**

(Paragraph 5.5.1 to 5.5.3. of this Regulation)



The label consists of a sticker which shall be weather resistant.

The centre zone indicates the first energy source.

The upper zone indicates the second energy source.

Layout and symbols shall be in accordance with ISO 17840-4:2018.

The colour and dimensions of the sticker shall fulfil the following requirements:

Colours:

Background: Orange, RGB code 255, 165, 0

Border: white or white reflecting

Letters: white or white reflecting

Dimensions:

Sticker width: 110 – 150 mm

Sticker height: 80 – 110 mm"

 II. Justification

1 Provisions for identification of gaseous and liquified fuels have been laid down in UN Regulations for LPG-fuelled M2/N2 and M3/N3 vehicles (UN Regulation No. 67, paragraph 17.1.8., including Annex 16 for details), CNG/LNG-fuelled M2/N2 and M3/N3 vehicles (UN Regulation No. 110, paragraph 18.1.8., including Annex 6 and 7 for the details) and Compressed Hydrogen-fuelled vehicles M2/N2 and M3/N3 vehicles (UN Regulation No. 134 paragraphs 7.1.7.1. and 7.1.7.3. including Annex 6 for the details).

2. The background for the additional labelling would help emergency services to determine how to approach these vehicles in case of a fire, especially the vehicle’s REESS.

3. For the installation of labels, this proposal seeks consistency with UN Regulation Nos. 67, 110 and 134.

4. CTIF [[3]](#footnote-4) recommends the use of symbols which are in line with the international standard **ISO 17840-4, Part 4 Propulsion energy identification**.

5. For the appearance of the label, this proposal seeks consistency with the above mentioned ISO standard.

1. \* In accordance with the programme of work of the Inland Transport Committee for 2023 as outlined in proposed programme budget for 2023 (A/77/6 (Sect. 20), table 20.6), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)
2. The latter number is given only as an example. [↑](#footnote-ref-3)
3. CTIF: historical abbreviation in French for *"Comité Technique International de prevention et d'extinction de Feu"*. [↑](#footnote-ref-4)