|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2023/59 | |
| _unlogo | **Economic and Social Council** | | Distr.: General  4 April 2023  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**190th session**

Geneva, 20-22 June 2023

Item 4.7.3. of the provisional agenda

**1958 Agreement:**

**Consideration of draft amendments to existing**

**UN Regulations submitted by GRPE**

Proposal for Supplement 8 to the 06 series of amendments to UN Regulation No. 49 (Emissions of compression ignition and positive ignition (LPG and CNG) engines)

Submitted by the Working Party on Pollution and Energy [[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on Pollution and Energy (GRPE) at its eighty-seventh session (ECE/TRANS/WP.29/GRPE/87, para. 49). It is based on ECE/TRANS/WP.29/GRPE/2023/5. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee (AC.1) for consideration at their June 2023 sessions.

*Annex 4*

*Paragraph 8.1.3.,* amend to read:

"8.1.3. Diluent

Formula for calculating the dry/wet correction factor based on the diluent humidity (21)

With

(22)

Where:

Hd is the diluent humidity, g water per kg dry air"

*Paragraph 8.6.3.,* amend to read:

"8.6.3. Calculation of the specific emissions

The specific emissions *e*gas or *e*PM (g/kWh) shall be calculated for each individual component in the following ways depending on the type of test cycle.

For the WHSC, hot WHTC, or cold WHTC, the following equation shall be applied:

 (69)

Where:

*m* is the mass emission of the component, g/test

*W*act is the actual cycle work as determined according to paragraph 7.8.6., kWh

For the WHTC, the final test result shall be a weighted average from cold start test and hot start test according to the following equation:

(70)

Where:

*m*cold is the mass emission of the component on the cold start test, g/test

*m*hot is the mass emission of the component on the hot start test, g/test

*W*act,cold is the actual cycle work on the cold start test, kWh

*W*act,hot is the actual cycle work on the hot start test, kWh

If periodic regeneration in accordance with paragraph 6.6.2. applies, the regeneration adjustment factors *k*r,u or *k*r,d shall be multiplied with or be added to, respectively, the specific emissions result *e* as determined in equations 69 and 70."

1. \* In accordance with the programme of work of the Inland Transport Committee for 2023 as outlined in proposed programme budget for 2023 (A/77/6 (Sect.20), para 20.6), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)