Proposal for Supplements from 03 to 08 series of amendments to UN Regulation No. 48

This document is a proposal to align from 03 to 08 series of amendments with 01 series of amendments to UN Regulations Nos.148 and 149. The modifications to the current text of the regulation are marked in bold for new and strikethrough for deleted characters.

I. Proposal

*Paragraph 5.10.4.3.,* amend to read:

"5.10.4.3. In case of doubt, the requirement above shall be deemed fulfilled if the luminous intensity of the red light emitted to the front and/or the white light emitted to the rear, as verified during type approval of the lamps, is ~~less~~ **not more** than 0.25 cd per lamp taking into account the influence of the vehicle body if applicable."

 II. Justification

1. This proposal aims to align the requirement for the visibility of red light towards the front and/or white light toward the rear of the vehicle from 03 to 08 series of amendments to UN Regulation No. 48 with 01 series of amendments to UN Regulations Nos. 148 and 149.
2. The objective test for the visibility of red light towards the front and/or white light toward the rear of the vehicle in case of doubt has already been added in all valid series of UN Regulation No. 48, from 03 to 08, along with the possibility of installation of lighting and light-signalling devices type-approved. Therefore, this technical correction needs be introduced accordingly.