Proposal for Supplements to 09 series of amendments

to UN Regulation No. 48

This document is a proposal to align the 09 series of amendments of UN Regulation No. 48 with 01 series of amendments to UN Regulations Nos.148 and 149. The modifications to the current text of the regulation are marked in bold for new and strikethrough for deleted characters.

I. Proposal

*Paragraph 5.10.4.3.,* amend to read:

"5.10.4.3. In case of doubt, the requirement above shall be deemed fulfilled if the luminous intensity of the red light emitted to the front and/or the white light emitted to the rear, as verified during type approval of the lamps, is ~~less~~ **not more** than 0.25 cd per lamp taking into account the influence of the vehicle body if applicable."

II. Justification

1. This proposal aims to align the requirement for the visibility of red light towards the front and/or white light toward the rear of the vehicle in 09 series of amendments to 01 series of amendments to UN Regulations Nos.148 and 149.