Proposal for Supplement 4 to the 05 Series of Amendments to UN Regulation No. 95 (Lateral impact) [[1]](#footnote-2)\*,[[2]](#footnote-3)\*\*

Submitted by the expert from France

The text reproduced below was prepared by the expert from France to clarify the figures of Annex 5 – Appendix 2 and reintroduce legends which had been removed in serie 2 of amendments of this regulation. The modifications to the current text of the UN Regulation are marked in bold for new characters.

1. Proposal

*Annex 5 – Appendix 2*, amend to read:

“Annex 5 – Appendix 2

FORCE-DEFLECTION CURVES FOR DYNAMIC TESTS

Figure 2a

Blocks 1 & 3

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | **Deflection** | | **Force** | |
|  |  |  |  |
| **A** | | | | **0** | **mm** | **10** | **kN** |
|  |
| **B** | | | | **300** | **mm** | **58** | **kN** |  |
|  |
| **C** | | | | **300** | **mm** | **43** | **kN** |  |
|  |
| **D** | | | | **30** | **mm** | **0** | **kN** |  |
|  |

**C**

**B**

**D**

**A**

Figure 2b

Block 2

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | **Deflection** | | **Force** | |
|  |  |  |  |
| **G** | | | | **0** | **mm** | **10** | **kN** |
|  |
| **H** | | | | **160** | **mm** | **70** | **kN** |  |
|  |
| **I** | | | | **160** | **mm** | **50** | **kN** |  |
|  |
| **J** | | | | **30** | **mm** | **0** | **kN** |  |
|  |

**I**

**H**

**J**

**G**

Figure 2c

Block 4

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | **Deflection** | | **Force** | |
|  |  |  |  |
| **K** | | | | **50** | **mm** | **5,0** | **kN** |
|  |
| **L** | | | | **300** | **mm** | **28,5** | **kN** |  |
|  |
| **M** | | | | **300** | **mm** | **18,5** | **kN** |  |
|  |
| **N** | | | | **80** | **mm** | **0** | **kN** |  |
|  |

**N**

**M**

**L**

**K**

Figure 2d

Blocks 5 & 6

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | **Deflection** | | **Force** | |
|  |  |  |  |
| **P** | | | | **50** | **mm** | **5,0** | **kN** |
|  |
| **Q** | | | | **300** | **mm** | **25,5** | **kN** |  |
|  |
| **R** | | | | **300** | **mm** | **15,5** | **kN** |  |
|  |
| **S** | | | | **80** | **mm** | **0** | **kN** |  |
|  |

Figure 2e

Blocks total

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | **Deflection** | | **Force** | |
|  |  |  |  |
| **T** | | | | **0** | **mm** | **25** | **kN** |
|  |
| **U** | | | | **160** | **mm** | **165** | **kN** |  |
|  |
| **V** | | | | **300** | **mm** | **255** | **kN** |  |
|  |
| **W** | | | | **300** | **mm** | **205** | **kN** |  |
|  |
| **X** | | | | **160** | **mm** | **115** | **kN** |  |
|  |
| **Y** | | | | **30** | **mm** | **0** | **kN** |  |
|  |

**“**

“

II. Justification

1. This proposal aims at clarifying the force-deflection curves of Annex 5 – Appendix 2. The force-deflection corridors characterising the rigidity of the impactor were described in the original serie of the UN Regulation No. 95 with a legend precising the value of the characteristics points of the curves (A to Y).



In the serie 2 of amendments, the figures were updated (without changing the corridors) and the legend were removed.

Une image contenant texte, ligne, capture d’écran, diagramme

Description générée automatiquement

This proposal aims at reintroducing the letters and the value in the legend for more clarity. The units of the deflection were also modified from cm to mm to be aligned with the units used in the rest of the text.

.

1. \* In accordance with the programme of work of the Inland Transport Committee for 2023 as outlined in proposed programme budget for 2023 (A/77/6 (Sect. 20), table 20.6), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)
2. \*\* This document was scheduled for publication after the standard publication date owing to circumstances beyond the submitter's control. [↑](#footnote-ref-3)