|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2015/86 |
|  | **Economic and Social Council** | Distr.: General24 August 2015Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**167th session**

Geneva, 10-13 November 2015

Item 4.7.5 of the provisional agenda

**1958 Agreement – Consideration of draft amendments**

**to existing Regulations submitted by GRSG**

Proposal for Supplement 3 to Regulation No. 61 (External projections of commercial vehicles)

**Submitted by the Working Party on General Safety Provisions**[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on General Safety Provisions (GRSG) at its 108th session (ECE/TRANS/WP.29/GRSG/87, para. 27). It is based on ECE/TRANS/WP.29/GRSG/2015/11. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee AC.1 for consideration at their November 2015 sessions.

*Paragraph 1.1.,* amend to read (including footnote 1):

"1.1. This Regulation applies to the external projections of goods vehicles of categories N1, N2 and N3 1, limited to the "external surface" as defined below. It does not apply to the exterior devices for indirect vision, including their support, or to the accessories such as aerials and luggage racks.

1 As defined in the Consolidated Resolution on the Construction of Vehicles (R.E.3.), document ECE/TRANS/WP.29/78/Rev.3, para. 2 - www.unece.org/trans/main/wp29/wp29wgs/wp29gen/wp29resolutions.html"

1. \* In accordance with the programme of work of the Inland Transport Committee for 2012–2016 (ECE/TRANS/224, para. 94 and ECE/TRANS/2012/12, programme activity 02.4), the World Forum will develop, harmonize and update Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)