Amendment to ECE/TRANS/WP.29/GRRF/2016/28

Agreed during the 82nd session

*…*

*Insert a new paragraph 4.8.*

"**4.8. Towing brackets / drawbeams which are intended to tow trailers up to 3.5t shall incorporate attachment points, to which either secondary couplings or devices necessary to enable the trailer to be guided and/or stopped automatically in the event of separation of the main coupling, may be attached.**

 **Other than for detachable units, as an alternative, an attachment point may be integrated to coupling component fitted to the towing bracket/drawbeam. The installation and operating instructions specified in 4.6. shall include all the information for the correct use these attachment points.**"

**…**