**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Joint Meeting of the RID Committee of Experts and the**

**Working Party on the Transport of Dangerous Goods 25. September 2017**

Geneva, 19–29 September 2017

Item 4 of the provisional agenda

**Harmonization with the United Nations**

**Recommendations on the Transport of Dangerous Goods**

 Disposition spéciale 671

 Transmitted by the Government of Belgium

 [Option 3:]« 671 Aux fins de la quantité totale maximale admissible par wagon ou grand conteneur / Aux fins des exemptions liées aux quantités transportées par unité de transport (voir 1.1.3.6), la catégorie de transport doit être déterminée en fonction du groupe d’emballage (voir troisième paragraphe de la disposition spéciale 251) :

- catégorie de transport 3 pour les trousses assignées au groupe d’emballage III ;

- catégorie de transport 2 pour les trousses assignées au groupe d’emballage II ;

- catégorie de transport 1 pour les trousses assignées au groupe d’emballage I ;

[Option 3:][“671 For the purposes of the total maximum permissible quantity per wagon or large container / exemption related to quantities carried per transport unit (see 1.1.3.6), the transport category shall be determined in relation to the packing group (see paragraph 3 of special provision 251):

- transport category 3 for kits assigned to packing group III;

- transport category 2 for kits assigned to packing group II;

- transport category 1 for kits assigned to packing group I;