|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2017/116/Corr.1 | |
| Description: _unlogo | **Economic and Social Council** | | Distr.: General  13 September 2017  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**173rd session**

Geneva, 14-17 November 2017

Item 4.7.6 of the provisional agenda

**1958 Agreement:  
Consideration of draft amendments**

**to existing Regulations submitted by GRSG**

Proposal for Supplement 2 to the 01 series of amendments to Regulation No. 121 (Identification of controls, tell-tales and indicators)

**Note by the secretariat [[1]](#footnote-2)\***

**Corrigendum**

**Page 2, Table 1**

Replace table with the table overleaf (keep the notes).

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *No.* | *Column 1* | *Column 2* | *Column 3* | *Column 4* | *Column 5* |
|  | *Item* | *Symbol 2* | *Function* | *Illumination* | *Colour* |
| … | … | … | … | … | … |
| 21. | Safety belt reminder | 18, 22 | Tell-tale | Yes | Red  22 |
| … | … | … | … | … | … |
| 31. | Combustion pre-heat;  engine start aid |  | Tell-tale | Yes | Yellow |
| 32. | Choke (cold starting device) |  | Control | No |  |
| … | … | … | … | … | … |
| 45 | Accident Emergency Call System (AECS) | or    21 | Control | Yes |  |
| Tell-tale |  |  |

1. \* In accordance with the programme of work of the Inland Transport Committee for 2016–2017 (ECE/TRANS/254, para. 159 and ECE/TRANS/2016/28/Add.1, cluster 3.1), the World Forum will develop, harmonize and update Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)