|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/GRRF/2017/4 | |
| Description: _unlogo | **Economic and Social Council** | | Distr.: General  10 November 2016  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**Working Party on Brakes and Running Gear**

**Eighty-third session**

Geneva, 23-27 January 2017

Item 7(c) of the provisional agenda

**Tyres: Regulation No. 54**

Proposal for amendments to Regulation No. 54 (Tyres for commercial vehicles and their trailers)

Submitted by the experts from the European Tyre and Rim Technical Organisation[[1]](#footnote-2)\*

The text reproduced below was prepared by the experts from the European Tyre and Rim Technical Organisation (ETRTO) in order to amend Annex 5 to Regulation No. 54. The modifications to the existing text of the Regulation are marked in bold for new or strikethrough for deleted characters.

1. Proposal

*Annex 5, part II, Table B,* add the following entries:

"

| *Tyre-size designation (+)* | *Measuring rim width code* | *Nominal rim diameter d (mm)* | *Outer diameter D (mm)* | | *Section width S (mm)* |
| --- | --- | --- | --- | --- | --- |
|  |  |  | *Normal* | *Snow* |  |
| **…**  **33x11.50R20LT**  **35x11.50R17LT**  **37x13.50R26LT**  **36x15.50R20LT**  **40x15.50R26LT**  **…** | **9.00**  **9.00**  **11.00**  **12.50**  **12.50** | **508**  **432**  **660**  **508**  **660** | **826**  **877**  **928**  **902**  **1004** | **832**  **883**  **934**  **908**  **1010** | **290**  **290**  **345**  **395**  **395** |

"

II. Justification

It is proposed to add these sizes as they are to be sold in countries requiring Type Approval according to Regulation No. 54.

1. \* In accordance with the programme of work of the Inland Transport Committee for 2010–2014 (ECE/TRANS/208, para. 106 and ECE/TRANS/2010/8, programme activity 02.4), the World Forum will develop, harmonize and update Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)