|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2019/95 | |
| _unlogo | **Economic and Social Council** | | Distr.: General  22 August 2019  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**179th session**

Geneva, 12-14 November 2019

Item 4.7.3 of the provisional agenda

**1958 Agreement:  
Consideration of draft amendments to existing   
UN Regulations submitted by GRSG**

Proposal for Supplement 9 to the 01 series of amendments to UN Regulation No. 43 (Safety glazing)

Submitted by the experts from the Working Party on General Safety[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on General Safety (GRSG) at its 116th session (ECE/TRANS/WP.29/GRSG/95, para. 25). It is based on ECE/TRANS/WP.29/GRSG/2019/5. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee (AC.1) for consideration at their November 2019 sessions.

Supplement 9 to the 01 series of amendments to UN Regulation No. 43 (Safety glazing)

*Annex 3, paragraph 6.4.1.3.,* amend to read:

"6.4.1.3. Procedure

Measure, according to paragraph 9.1. of this annex, the luminous transmission of the test specimen(s) to be exposed. That face of each test pieces, which would represent the surface glazed to the exterior of the road vehicle, shall face the lamp. Other exposure conditions shall be as follows:

……"

1. \* In accordance with the programme of work of the Inland Transport Committee for 2018–2019 (ECE/TRANS/274, para. 123 and ECE/TRANS/2018/21/Add.1, Cluster 3.1), the World Forum will develop, harmonize and update UN regulations to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)