Draft Proposed amendments to ECE/TRANS/WP.29/2019/120

1. Proposal

*Paragraph 6.3.3.(g), amend to read:*

“(g) Excessive ~~visual~~ **visible** smoke emission;

*Paragraph 6.4.2.4.(s), amend to read:*

“(g) ~~Visual~~ **Visible** smoke emission, **black soot deposit in the exhaust pipe (for vehicles equipped with a particulate filter)** or unobtrusive drive-by emissions measurement;;

*Paragraph 6.5.3.(a), amend to read:*

“(a) Vehicles identified as gross polluters by means of remote sensing techniques**,** ~~or~~ emitting excessive ~~visual~~ **visible** smoke **or black soot deposit in the exhaust pipe (for vehicles equipped with a particulate filter)**;

1. Justification

If a particulate filter is defective and/or has been removed, soot deposit are likely to appear on the exhaust pipe, highlighting a potential problem with the particulate filter.