UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council

TRANS/WP.29/2001/48

21 August 2001

ENGLISH

Original:	ENGLISH

and FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

World Forum for Harmonization of Vehicle Regulations (WP.29)

(One-hundred-and-twenty-fifth session,

6-9 November 2001, agenda item 5.2.13.)

PROPOSAL FOR DRAFT SUPPLEMENT 3 TO REGULATION No. 65

(Special warning lamps)

Transmitted by the Working Party on Lighting

and Light-Signalling (GRE)

Note: The text reproduced below was adopted by GRE at its forty-fifth session, however, a decision concerning its transmission for consideration to WP.29 and AC.1 has only been taken at the forty-sixth session. It is based on document TRANS/WP.29/GRE/2000/13, not amended (TRANS/WP.29/GRE/45, para. 31; TRANS/WP.29/GRE/46, para. 32). The presentation of the trichromatic coordinates was aligned with that used in Regulation No. 65.

__________

This document is a working document circulated for discussion and comments.

The use of this document for other purposes is the entire responsibility of the user. Documents are also available via the INTERNET:

http://www.unece.org/trans/main/welcwp29.htm

GE.01-

Annex 3, amend to read:

"...... shall lie within the following boundaries:

1. Amber */

limit towards green	:	y ≤ x - 0.120

limit towards red	:	y ≥ 0.390

limit towards white	:	y ≤ 0.790 - 0.670 x

2. Blue

........"

___________