UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/738
31 August 2000

ENGLISH

Original: ENGLISH

and FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

World Forum for Harmonization of Vehicle Regulations (WP.29)

DRAFT SUPPLEMENT 13 TO REGULATION No. 54

(Pneumatic tyres for commercial vehicles)

Note: The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its fifteenth session, following the recommendation by WP.29 at its one-hundred-and-twenty-first session. It is based on document TRANS/WP.29/2000/37, not amended (TRANS/WP.29/735, para. 116).

__________

GE.00-

Annex 5, Part II, Table B, insert at the end the following new tyre size:

"

Tyre size

designation

1/	Measuring rim width code	Nominal rim diameter d(mm)	Outer diameter D(mm) 2/

Normal Snow	Section width S(mm) 3/
..........

37x12.50 R 17LT	...........

10.00	...........

432	.....

928	.....

934	...........

318

"

____________