Proposal for amendments to
ECE-TRANS-WP.29/GRVA/2021/03

 This document supplements the proposed provisions for the extension of the scope of ALKS including all vehicle categories M and N per ECE/TRANS/WP.29/
GRVA/2021/03. The modifications of the existing Regulation are marked in bold for new.

1. **Proposal**

*Paragraph 8.4.3.*, amend to read (including a new footnote X):

“8.4.3. The data shall be retrievable even after an impact of a severity level set by UN Regulations Nos. 94, 95 or 137 **for vehicles of Category M1 and N1, UN Regulation No. 29 for N2/N3 and UN Regulation No. 66 for M2/M3x, as applicable.** If the main on-board vehicle power supply is not available, it shall still be possible to retrieve all data recorded on the DSSAD, as required by national and regional law.”

*Add a new footnote X*, to read:

“**x The manufacturer shall provide the Technical Service with the documentation and supporting evidence to demonstrate compliance with these provisions. This information shall be subject to discussion and agreement between the Technical Service and vehicle manufacturer.**”

1. **Justification**

 As UN Regulations Nos. 94, 95 or 137 refer only to vehicle categories M1 and N1, the extension to UN Regulations Nos. 29 and 66 will set an impact of a severity level also for the other vehicle categories.