|  |  |  |
| --- | --- | --- |
|  | United Nations | ST/SG/AC.10/C.3/2021/29 |
| _unlogo | **Secretariat** | Distr.: General18 May 2021EnglishOriginal: English and French |

**Committee of Experts on the Transport of Dangerous Goods
and on the Globally Harmonized System of Classification
and Labelling of Chemicals**

**Sub-Committee of Experts on the Transport of Dangerous Goods**

**Fifty-eighth session**

Geneva, 28 June-2 July

Item 6 (d) of the provisional agenda

**Miscellaneous proposals for amendments to the Model Regulations
on the Transport of Dangerous Goods: other miscellaneous proposals**

 Editorial amendments

 Note by the secretariat[[1]](#footnote-2)

 I. Introduction

1. From 21 to 23 April 2021, the Ad Hoc Working Group on the Harmonization of RID/ADR/ADN with the UN Recommendations on the Transport of Dangerous Goods met virtually. During their discussions, a few potential amendments to the Model Regulations were identified. These are collected below in proposals 1 (amendments) and 2 (corrections).

2. Furthermore, the secretariat has either identified or been made aware of other issues which are collected in proposal 3 below.

3. The Sub-Committee may wish to consider the following proposals for adoption.

 II. Proposal 1 (amendments from the Harmonization Ad Hoc Working Group)

1.2.1 The amendment does not apply to the English version.

***Note from the secretariat:*** *The Sub-Committee may want to consider whether the meaning of the word “content” in item (b) of the definition of “Working pressure” needs to be clarified.*

2.4.2.3.2.3 Replace “The formulations not listed in this provision” by “The formulations not listed in this sub-section”.

2.5.3.2.4 Replace “The formulations not listed in this provision” by “The formulations not listed in this sub-section”.

3.3, SP 396 (f) Replace “and are marked” by “and marked”.

4.1.3.3 In the last sentence, replace “packages” by “packagings”.

4.1.4.1, P200 (5) ***Note from the secretariat:*** *The Sub-Committee may want to consider if the use of “abs.” (twice) is appropriate or if it should be removed or substituted by “absolute”.*

4.1.4.2, IBC520 Replace “the formulations not listed in 2.4.2.3.2.3 and 2.5.3.2.4” by “the formulations not listed in 2.4.2.3.2.3 or 2.5.3.2.4”.

4.2.5.2.6, T23 Replace “the formulations not listed in 2.4.2.3.2.3 and 2.5.3.2.4” by “the formulations not listed in 2.4.2.3.2.3 or 2.5.3.2.4”.

6.2.1.5.2 After (p), replace “closed cryogenic pressure receptacles” by “closed cryogenic receptacles”.

6.2.1.5.4 In the second sentence, replace “weight” by “mass”.

6.2.2.7.3 (l) (ii) After “porous material”, add “(e.g.: name or trademark)”.

6.9.2.2.3.14.1 Delete “of Class 3”.

 III. Proposal 2 (corrections from the Harmonization Ad Hoc Working Group)

**Chapter 6.5, 6.5.6.3.2**

*For* 6.5.5.4.9 *read* 6.5.5.4.8

**Chapter 6.9, 6.9.2.3.4, indent K₄, sub-indent 1.0**

*For* 6.9.2.7.1.2 (i) *read* 6.9.2.7.1.2 (h)

**Chapter 6.9, 6.9.2.7.1.2 (e)**

*For* 6.9.2.2.4 *read* 6.9.2.2.3.2

**Chapter 6.9, 6.9.2.7.1.2 (f)**

*For* 6.9.2.2.4 *read* 6.9.2.2.3.2

 IV. Proposal 3 (other corrections)

**Chapter 1.5, 1.5.2.5, first sentence**

*For* persons *read* people

 **Chapter 2.5, 2.5.3.2.4, entry for “ISOPROPYL sec-BUTYL PEROXYDICARBONATE+DI-sec-BUTYL PEROXYDICARBONATE+DI-ISOPROPYL PEROXYDICARBONATE”, column “Concentration”**

*For* ≤ 32 + ≤ 15 – 18 ≤ 12 -15 *read* ≤ 32 + ≤ 15 – 18 + ≤ 12 -15

**Chapter 6.2, 6.2.1.6.1 (d), note 3**

For the existing text, *substitute*

NOTE 3: The check of internal conditions of 6.2.1.6.1 (b) and the hydraulic pressure test of 6.2.1.6.1 (d) may be replaced by ultrasonic examination carried out in accordance with ISO 18119:2018 for seamless steel and seamless aluminium alloy cylinder shells. For a transitional period until 31 December 2024 the standard ISO 10461:2005 +A1:2006 may be used for seamless aluminium alloy cylinder shells and ISO 6406:2005 may be used for seamless steel cylinder shells for this same purpose.

1. A/75/6 (Sect.20), para. 20.51 [↑](#footnote-ref-2)