|  |  |  |
| --- | --- | --- |
|  |  | **UN/SCETDG/58/INF.44** |

|  |
| --- |
| **Committee of Experts on the Transport of Dangerous Goods  and on the Globally Harmonized System of Classification and Labelling of Chemicals 30 June 2021** |
| **Sub-Committee of Experts on the Transport of Dangerous Goods**  **Fifty-eighth session**  Geneva, 28 June-2 July 2021 Item 14 of the provisional agenda  **Other business** |

Classification of UN 1010, mixtures of Butadienes and Hydrocarbons

Transmitted by the European Chemical Industry Council (Cefic)

Additional proposals on document ST/SG/AC.10/C.3/2021/22 and informal document INF.40 from Cefic

1. Based on the discussion of the Sub-Committee on Classification of UN 1010, we would like to amend our proposal as follows:
2. In 3.2 replace “UN 1010 BUTADIENES, STABILIZED or BUTADIENES AND HYDROCARBON MIXTURE, STABILIZED, containing more than 40 % butadienes” by “UN 1010 BUTADIENES, STABILIZED or BUTADIENES AND HYDROCARBON MIXTURE, STABILIZED, containing more than 20 % butadienes”
3. Insert a new Special Provision SPXX:

“Substances transported under this entry shall have a vapour pressure at 70 °C not exceeding 1.1 MPa (11 bar) and a density at 50 °C not lower than 0.525 kg/l”

1. Consequential amendments:

The proper shipping name for UN 1010 in packing instruction P200, Table 2 should be amended accordingly.