|  |  |  |
| --- | --- | --- |
|  | E/ECE/324/Rev.1/Add.15/Rev.9/Amend.7−E/ECE/TRANS/505/Rev.1/Add.15/Rev.9/Amend.7 | |
|  |  | 2 July 2021 |

Agreement

Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

(Revision 3, including the amendments which entered into force on 14 September 2017)

\_\_\_\_\_\_\_\_\_

Addendum 15 – UN Regulation No. 16

Revision 9 - Amendment 7

Supplement 6 to the 07 series of amendments – Date of entry into force: 9 June 2021

Uniform provisions concerning the approval of:

I. Safety-belts, restraint systems, child restraint systems and ISOFIX child restraint systems for occupants of power-driven vehicles

II. Vehicles equipped with safety-belts, safety-belt reminder, restraint systems, child restraint systems, ISOFIX child restraint systems and i-Size child restraint systems

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2020/112 (as amended by paragraph 102 of the report ECE/TRANS/WP.29/1155).

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Paragraph 8.4.4.2.*, amend to read:

"8.4.4.2. The visual warning shall indicate at least all rear seating positions to allow the driver to identify, while facing forward as seated on the driver seat, any seating position in which the safety-belt is unfastened. For vehicles that have information on the occupancy status of the rear seats, the visual warning does not need to indicate unfastened safety-belts for unoccupied seating positions. For seats, which can be fixed to different designated seating positions within the vehicle (e.g. floor rail mounted), the visual warning shall at least indicate when any rear safety-belt is unfastened."

1. \* Former titles of the Agreement:

   Agreement concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

   Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)