|  |  |  |
| --- | --- | --- |
|  | E/ECE/324/Rev.2/Add.120/Rev.2/Amend.4−E/ECE/TRANS/505/Rev.2/Add.120/Rev.2/Amend.4 | |
|  |  | 2 November 2020 |

Agreement

Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

(Revision 3, including the amendments which entered into force on 14 September 2017)

\_\_\_\_\_\_\_\_\_

Addendum 120 – UN Regulation No. 121

Revision 2 - Amendment 4

Supplement 4 to the 01 series of amendments — Date of entry into force: 25 September 2020

Uniform provisions concerning the approval of vehicles with regard to the location and identification of hand controls, tell-tales and indicators

This document is meant purely as documentation tool. The authentic and legal binding texts is: ECE/TRANS/WP.29/2020/22.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Table 1*, amend to read (adding the references to footnote 18):

"

| *No.* | *Column 1* | *Column 2* | *Column 3* | *Column 4* | *Column 5* |
| --- | --- | --- | --- | --- | --- |
|  | *Item* | *Symbol* ***2*** | *Function* | *Illumination* | *Colour* |
|  | … |  |  |  |  |
| 7. | Front fog lamps |  | Control | No |  |
|  |  | 1**, 18** | Tell-tale | Yes | Green |
| 8. | Rear fog lamp |  | Control | No |  |
|  |  | 1**, 18** | Tell-tale | Yes | Yellow |
|  | … |  |  |  |  |
| 17. | Windscreen defrosting and defogging system  (with separate operating control) | **18** | Control | Yes |  |
|  |  |  | Tell-tale | Yes | Yellow |
| 18. | Rear window defrosting and defogging system  (with separate operating control) | **18** | Control | Yes |  |
|  |  |  | Tell-tale | Yes | Yellow |
|  | … |  |  |  |  |
| 20. | Parking lamps | **18** | Control | No |  |
| Tell-tale | Yes | Green |
|  | … |  |  |  |  |
| 31. | Diesel pre-heat | **18** | Tell-tale | Yes | Yellow |
| 32. | Choke (cold starting device) | **18** | Control | No |  |
| Tell-tale |  | Yellow |
|  | … |  |  |  |  |

…

18 Symbol may be shown in other colours than specified in column 5 in order to convey different meanings according to the general colour coding as proposed in paragraph 5 of ISO 2575-2004.

… "

1. \* Former titles of the Agreement:

   Agreement concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

   Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)