|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.15/AC.2/2022/23 | |
| Description: _unlogo | **Economic and Social Council** | | Distr.: General  16 May 2022  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Joint Meeting of Experts on the Regulations annexed to the   
European Agreement concerning the International Carriage   
of Dangerous Goods by Inland Waterways (ADN)**

**(ADN Safety Committee)**

**Fortieth session**

Geneva, 22–26 August 2022

Item 4 (a) of the provisional agenda

**Proposals for amendments to the Regulations annexed to ADN:**

**work of the RID/ADR/ADN Joint Meeting**

Changes to Table B in ADN 2023

Note by the secretariat [[1]](#footnote-2)\*, [[2]](#footnote-3)\*\*

Introduction

1. The alphabetic index of substances and articles in Table B of ADN does not form an integral part of ADN. Therefore, the changes to Table B adopted by the RID/ADR/ADN Joint Meeting and the Working Party on the Transport of Dangerous Goods (WP.15) are not reproduced in the consolidated list of draft amendments to ADN (ECE/ADN/61).

2. A summary of these changes is given below for information of the ADN Safety Committee in alphabetical order.

List of changes

**Chapter 3.2**

3.2.2 In Note 1, after “tert”;”, add “the prefixes “cis” and “trans”;”.

*(Reference document: ECE/TRANS/WP.15/AC.1/2021/24/Add.1)*

**Chapter 3.2, Table B**

In the entry for “AMMONIUM NITRATE, LIQUID, hot concentrated solution, in a concentration of more than 80% but not more than 93%”, amend column “Name and description” to read: “AMMONIUM NITRATE, LIQUID (hot concentrated solution)”.

*(Reference document: ECE/TRANS/WP.15/253)*

Amend the entry for “BUTYLENES MIXTURE or 1-BUTYLENE or CIS-2-BUTYLENE or TRANS-2-BUTYLENE” to read as follows:

|  |  |  |
| --- | --- | --- |
| BUTYLENE | 1012 | 2 |

Amend the entry for “EXTRACTS, AROMATIC, LIQUID” to read as follows:

|  |  |  |
| --- | --- | --- |
| Extracts, aromatic, liquid, see | 1197 | 3 |

Amend the entry for “EXTRACTS, FLAVOURING, LIQUID” to read as follows:

|  |  |  |
| --- | --- | --- |
| Extracts, flavouring, liquid, see | 1197 | 3 |

In the entry “RUBBER SCRAP, powdered or granulated”, amend column “Name and description” to read:

“RUBBER SCRAP, powdered or granulated, not exceeding 840 microns and rubber content exceeding 45 %”.

*(Reference document: ECE/TRANS/WP.15/251)*

In the entry “RUBBER SHODDY, powdered or granulated”, amend column “Name and description” to read:

“RUBBER SHODDY, powdered or granulated, not exceeding 840 microns and rubber content exceeding 45 %”.

*(Reference document: ECE/TRANS/WP.15/251)*

Add the following new entries in alphabetical order:

|  |  |  |
| --- | --- | --- |
| 1-butylene, see | 1012 | 2 |
| cis-2-butylene, see | 1012 | 2 |
| trans-2-butylene, see | 1012 | 2 |
| Butylenes, mixture, see | 1012 | 2 |
| COBALT DIHYDROXIDE POWDER, containing not less than 10 % respirable particles | 3550 | 6.1 |
| EXTRACTS, LIQUID, for flavour or aroma | 1197 | 3 |
| HYDROGEN PEROXIDE, STABILIZED | 2015 | 5.1 |

1. \* Distributed in German by the Central Commission for the Navigation of the Rhine under the symbol CCNR-ZKR/ADN/WP.15/AC.2/2022/23 [↑](#footnote-ref-2)
2. \*\* A/76/6 (Sect.20), para. 20.76. [↑](#footnote-ref-3)