|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2022/103 |
| _unlogo | **Economic and Social Council** | Distr.: General7 April 2022Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**187th session**

Geneva, 21-24 June 2022

Item 4.14.15 of the provisional agenda

**1958 Agreement:
Pending proposals for amendments to existing UN Regulations submitted by GRE and GRSG**

 Proposal for Supplement 4 to the 01 series of amendments to UN Regulation No. 86 (Installation of lighting and light-signalling devices for agricultural vehicles)

 Submitted by the Working Party on Lighting and Light-Signalling[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on Lighting and Light-Signalling (GRE) at its eighty-fifth session2 (ECE/TRANS/WP.29/GRE/85, para. 26). It is based on ECE/TRANS/WP.29/GRE/2021/22. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee (AC.1) for consideration at their June 2022 sessions.

*Paragraph 6.1.2.,* amend to read:

"6.1.2. Number: Two, type‑approved according to:

 - UN Regulations Nos. 98 or 112 or 113,

 or

- Classes A, B, BS, CS, D, DS or ES of the 00 series of amendments to UN Regulation No. 149,

or

- Classes A, B, BS, CS or DS of the 01 and subsequent series of amendments to UN Regulation No. 149.

 Optionally one additional pair type‑approved according to:

 - UN Regulations Nos. 98 or 112 or 113,

 or

 - Classes A, B, BS, CS, D, DS or ES of the 00 series of amendments to UN Regulation 149,

 or

 - Classes A, B, BS, CS, DS or RA of the 01 and susbsequent series of amendments to UN Regulation No. 149."

*Paragraph 6.1.9.2.,* amend to read:

"6.1.9.2. This maximum intensity shall be obtained by adding together the individual reference marks which are indicated on the several headlamps."

*Paragraph 6.2.2.,* amend to read:

"6.2.2. Number: Two (or four - see paragraph [6.2.4.2.4.](http://srace2:8080/document/show/document_id/1771#A0_S6_2_3_2_1_)), type‑approved according to

 - UN Regulations Nos. 98 or 112 or 113,

 or

 - Classes A, AS, B, BS, CS, D, DS or ES of the 00 series of amendments to UN Regulation No. 149,

 or

 - Classes AS, BS, C, CS, DS or V of the 01 and subsequent series of amendments to UN Regulation No. 149."

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. \* In accordance with the programme of work of the Inland Transport Committee for 2022 as outlined in proposed programme budget for 2022 (A/76/6 (part V sect. 20) para 20.76), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)