|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/ADN/61/Add.1 | |
| _unlogo | **Economic and Social Council** | | Distr.: General  26 August 2022  English  Original: English and French |

**Economic Commission for Europe**

**Administrative Committee of the European Agreement   
Concerning the International Carriage of Dangerous  
Goods by Inland Waterways (ADN)**

European Agreement concerning the International Carriage of Dangerous Goods by Inland Waterways (ADN)

Draft amendments to the Regulations annexed to ADN[[1]](#footnote-2)\*

Addendum

Chapter 1.2

1.2.1 After the definition of “Tank-container”, insert:

“In addition:

*"Extra-large tank-container"* means a tank-container with a capacity of more than 40 000 litres.”

Chapter 1.6

1.6.1 Add the following new transitional measures:

“1.6.1.52 Inner receptacles of composite IBCs manufactured before 1 July 2021 in accordance with the requirements of 6.5.2.2.4 of ADR in force up to 31 December 2020 and which are not in accordance with the requirements of 6.5.2.2.4 of ADR regarding the marks on the inner receptacles that are not readily accessible for inspection due to the design of the outer casing applicable as from 1 January 2021 may continue be used until the end of their period of use determined in 4.1.1.15 of ADR.”

“1.6.1.53 *(Reserved)*”

Chapter 1.8

1.8.5.4 In the “Model report on occurrences during the carriage of dangerous goods”, section 6, note (3), add a new entry to read “18 Extra-large tank-container”. Renumber remaining entries accordingly.

Chapter 1.10

1.10.4 Delete the first sentence. In the second sentence, replace “In addition, the provisions” by “The provisions”.

**Chapter 3.2, Table A**

Add the following new entry:

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| (1) | (2) | (3a) | (3b) | (4) | (5) | (6) | (7a) | (7b) | (8) | (9) | (10) | (11) | (12) | (13) |
| 3550 | COBALT DIHYDROXIDE POWDER, containing not less than 10 % respirable particles | 6.1 | T5 | I | 6.1 | 802 | 0 | E5 |  | PP, EP |  |  | 2 |  |

Chapter 5.4

5.4.2 In footnote 6, first sentence, replace “Amendment 39-18” by “Amendment 40-20”.

In footnote 6, in the text reproducing section 5.4.2 of the IMDG Code:

5.4.2.2 At the end of the first sentence, delete “one to the other”.

5.4.2.3 The amendment doesn’t apply to the English text.

5.4.2.4 The amendment doesn’t apply to the English text.

1. \* Distributed in German by the Central Commission for the Navigation of the Rhine under the symbol CCNR/ZKR/ADN/61/Add.1. [↑](#footnote-ref-2)