|  |  |  |
| --- | --- | --- |
|  | E/ECE/324/Add.9/Rev.6/Amend.2−E/ECE/TRANS/505/Add.9/Rev.6/Amend.2 | |
|  |  | 11 November 2022 |

Agreement

Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

(Revision 3, including the amendments which entered into force on 14 September 2017)

\_\_\_\_\_\_\_\_\_

Addendum 9 – UN Regulation No. 10

Revision 6 - Amendment 2

Supplement 2 to the 06 series of amendments – Date of entry into force: 8 October 2022

Uniform provisions concerning the approval of vehicles with regard to electromagnetic compatibility

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2022/33.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Annex 4 - Appendix 1,*

*Figure 1,* amend to read:

"Figure 1

Clear horizontal surface free of electromagnetic reflection delimitation

of the surface defined by an ellipse

Vehicle axis positioned on   
normal from antenna midpoint

Vehicle under test

Centre of 30 m radius   
(20 m for 3 m measurements)  
clear area at midpoint   
between reference antenna   
and nearest part of the  
vehicle body

Reference antenna

15 m min radius  
(10 m for 3 m measurements)

Permitted region for

measuring equipment

(in hut or vehicle)

10,0 m ± 0,2 m  
(3,00 m ± 0,05 m   
for 3 m measurements)

*Annex 6,*

*Paragraph 3.3.4.,* amend to read:

"3.3.4. Either at 1.0 ± 0.2 m behind the vertical centreline of the vehicle's front wheel(s) (point C in Figure 1 of Appendix 1 to this annex) in the case of three-wheeled or four-wheeledvehicles.

Or at 0.2 ± 0.2 m behind the vertical centreline of the vehicle's front wheel (point D in Figure 2 of Appendix 1 to this annex) in the case of two-wheeled vehicles."

1. \* Former titles of the Agreement:

   Agreement concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

   Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)