1958 Agreement - Unique Identifier
Review of UN Regulations under the purview of GRE

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ***No.***  | ***Title*** | ***Use of UI prohibited*** | ***Use of UI possible***  | ***Remarks*** |
| ***Is there additional information required in the approval mark[[1]](#footnote-2)(Yes/No)*** | ***Summary document necessary (Yes/No)*** | ***Should additional physical marking remain on the product (Yes/No)?******In case of yes, which one(s)?*** | ***E.g. justifications for additional physical markings that must remain on the product*** |
|  1 | Uniform provisions concerning the approval of motor vehicle headlamps emitting an asymmetrical passing-beam and/or a driving-beam and equipped with filament lamps of categories R2 and/or HS1 |  |  |  |  |  |
|  2 | Uniform provisions concerning the approval of incandescent electric lamps for headlamps emitting an asymmetrical passing-beam or a driving-beam or both |  |  |  |  |  |
|  3 | Uniform provisions concerning the approval of retro-reflecting devices for power-driven vehicles and their trailers |  |  |  |  |  |
|  4 | Uniform provisions concerning the approval of devices for the illumination of rear registration plates of power-driven vehicles and their trailers |  |  |  |  |  |
|  5 | Uniform provisions concerning the approval of power-driven vehicle's "sealed beam" headlamps (SB) emitting a European asymmetrical passing-beam or a driving-beam or both |  |  |  |  |  |
|  6 | Uniform provisions concerning the approval of direction indicators for power-driven vehicles and their trailers |  |  |  |  |  |
|  7 | Uniform provisions concerning the approval of front and rear position lamps, stop-lamps and end-outline marker lamps for motor vehicles and their trailers |  |  |  |  |  |
|  8 | Uniform provisions concerning the approval of motor vehicle headlamps emitting an asymmetrical passing-beam or a driving-beam or both and equipped with halogen filament lamps (H1, H2, H3, HB3, HB4, H7, H8, H9, HIR1, HIR2 and/or H11) |  |  |  |  |  |
| 10 | Uniform provisions concerning the approval of vehicles with regard to electromagnetic compatibility |  |  |  |  |  |
| 19 | Uniform provisions concerning the approval of power-driven vehicle front fog lamps |  |  |  |  |  |
| 20 | Uniform provisions concerning the approval of motor vehicle headlamps emitting an asymmetrical passing-beam or a driving-beam or both and equipped with halogen filament lamps (H4 lamps) |  |  |  |  |  |
| 23 | Uniform provisions concerning the approval of reversing and manoeuvring lamps for power-driven vehicles and their trailers |  |  |  |  |  |
| 27 | Uniform provisions concerning the approval of advance-warning triangles |  |  |  |  |  |
| 31 | Uniform provisions concerning the approval of power-driven vehicle's halogen sealed-beam headlamps (HSB) emitting a European asymmetrical passing-beam or a driving-beam or both |  |  |  |  |  |
| 37 | Uniform provisions concerning the approval of filament light sources for use in approved lamps of power-driven vehicles and of their trailers |  |  |  |  |  |
| 38 | Uniform provisions concerning the approval of rear fog lamps for power-driven vehicles and their trailers |  |  |  |  |  |
| 45 | Uniform provisions concerning the approval of headlamp cleaners, and of power-driven vehicles with regard to headlamp cleaners |  |  |  |  |  |
| 48 | Uniform provisions concerning the approval of vehicles with regard to the installation of lighting and light-signalling devices |  |  |  |  |  |
| 50 | Uniform provisions concerning the approval of front position lamps, rear position lamps, stop lamps, direction indicators and rear-registration-plate illuminating devices for vehicles of category L |  |  |  |  |  |
| 53 | Uniform provisions concerning the approval of category L3 vehicles with regard to the installation of lighting and light-signalling devices |  |  |  |  |  |
| 56 | Uniform provisions concerning the approval of headlamps for mopeds and vehicles treated as such |  |  |  |  |  |
| 57 | Uniform provisions concerning the approval of headlamps for motorcycles and vehicles treated as such |  |  |  |  |  |
| 65 | Uniform provisions concerning the approval of special warning lamps for power-driven vehicles and their trailers |  |  |  |  |  |
| 69 | Uniform provisions concerning the approval of rear marking plates for slow-moving vehicles (by construction) and their trailers |  |  |  |  |  |
| 70 | Uniform provisions concerning the approval of rear marking plates for heavy and long vehicles |  |  |  |  |  |
| 72 | Uniform provisions concerning the approval of motorcycle headlamps emitting an asymmetrical passing-beam and a driving-beam and equipped with halogen lamps (HS1 lamps) |  |  |  |  |  |
| 74 | Uniform provisions concerning the approval of category L1 vehicles with regard to the installation of lighting and light-signalling devices |  |  |  |  |  |
| 76 | Uniform provisions concerning the approval of headlamps for mopeds emitting a driving-beam and a passing-beam |  |  |  |  |  |
| 77 | Uniform provisions concerning the approval of parking lamps for power-driven vehicles |  |  |  |  |  |
| 82 | Uniform provisions concerning the approval of moped headlamps equipped with filament halogen lamps (HS2) |  |  |  |  |  |
| 86 | Uniform provisions concerning the approval of agricultural or forestry vehicles with regard to the installation of lighting and light-signalling devices |  |  |  |  |  |
| 87 | Uniform provisions concerning the approval of daytime running lamps for power-driven vehicles |  |  |  |  |  |
| 88 | Uniform provisions concerning the approval of retroreflective tyres for two-wheeled vehicles |  |  |  |  |  |
| 91 | Uniform provisions concerning the approval of side-marker lamps for motor vehicles and their trailers |  |  |  |  |  |
| 98 | Uniform provisions concerning the approval of motor vehicle headlamps equipped with gas-discharge light sources |  |  |  |  |  |
| 99 | Uniform provisions concerning the approval of gas-discharge light sources for use in approved lamps of power-driven vehicles |  |  |  |  |  |
| 104 | Uniform provisions concerning the approval of retro-reflective markings for vehicles of category M, N and O |  |  |  |  |  |
| 112 | Uniform provisions concerning the approval of motor vehicle headlamps emitting an asymmetrical passing-beam or a driving-beam or both and equipped with filament lamps and/or Light-Emitting Diode (LED) modules |  |  |  |  |  |
| 113 | Uniform provisions concerning the approval of motor vehicle headlamps emitting a symmetrical passing-beam or a driving-beam or both and equipped with filament, gas-discharge light sources or LED modules |  |  |  |  |  |
| 119 | Uniform provisions concerning the approval of cornering lamps for power-driven vehicles |  |  |  |  |  |
| 123 | Uniform provisions concerning the approval of adaptive front-lighting systems (AFS) for motor vehicles |  |  |  |  |  |
| 128 | Uniform provisions concerning the approval of Light Emitting Diode (LED) light sources for use in approved lamps on power-driven vehicles and their trailers |  |  |  |  |  |
| 148 | Uniform provisions concerning the approval of light-signalling devices (lamps) for power-driven vehicles and their trailers |  |  |  |  |  |
| 149 | Uniform provisions concerning the approval of road illumination devices (lamps) and systems for power-driven vehicles |  |  |  |  |  |
| 150 | Uniform provisions concerning the approval of retro-reflective devices and markings for power-driven vehicles and their trailers |  |  |  |  |  |

1. A circle surrounding the letter "E" followed by the distinguishing number of the country which has granted approval. The approval number. The number of this Regulation followed by the letter 'R' and the two digits indicating the series of amendments in force at the time of issue of the approval. [↑](#footnote-ref-2)