|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.15/AC.2/2023/26 | |
| United Nations logo | **Economic and Social Council** | | Distr.: General  17 May 2023  English  Original: French |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Joint Meeting of Experts on the Regulations annexed to the**

**European Agreement concerning the International Carriage**

**of Dangerous Goods by Inland Waterways (ADN)**

**(ADN Safety Committee)**

**Forty-second session**

Geneva, 21–25 August 2023

Item 4 (b) of the provisional agenda

**Proposals for amendments to the Regulations annexed to ADN:**

**Other proposals**

8.1.6.2 of ADN: Checking and inspection of equipment – Hose assemblies

Transmitted by the Government of Germany[[1]](#footnote-1)\*, [[2]](#footnote-2)\*\*

Introduction

1. In 8.1.6.2, since 1 January 2023, the first sentence mentions ISO standard 13765:2018:

“... ISO 13765:2018 (thermoplastic multilayer (non-vulcanized) hoses and hose assemblies) ...”

2. However, the second sentence refers to an EN standard with the same number.

3. The first sentence contains an editorial error which first occurred in the amendment transmitted by the German delegation in document ECE/TRANS/WP.15/AC.2/2022/4 of 10 November 2021, paragraph 103. ISO standard 13765 covers refractory mortars, which are not relevant to ADN. However, EN standard 13765 does cover thermoplastic hoses and hose assemblies.

4. In 1.6.7.2.2.2, the relevant transitional provision for 8.1.6.2 mentions “EN ISO 13765:2018”. There is no such EN and ISO standard 13765 with identical content.

Request for amendment

5. In 8.1.6.2, first sentence, replace “ISO 13765:2018” with “EN 13765:2018”.

6. In 1.6.7.2.2.2, in the line for 8.1.6.2, second column, replace “EN ISO 13765:2018” with “EN 13765:2018”.

1. \* Distributed in German by the Central Commission for the Navigation of the Rhine under the symbol CCNR-ZKR/ADN/WP.15/AC.2/2023/26. [↑](#footnote-ref-1)
2. \*\* A/77/6 (Sect. 20), table 20.6. [↑](#footnote-ref-2)