|  |  |  |
| --- | --- | --- |
|  | E/ECE/324/Rev.2/Add.120/Rev.2/Amend.6−E/ECE/TRANS/505/Rev.2/Add.120/Rev.2/Amend.6 | |
|  |  | 28 November 2023 |

Agreement

Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

(Revision 3, including the amendments which entered into force on 14 September 2017)

\_\_\_\_\_\_\_\_\_

Addendum 120 – UN Regulation No. 121

Revision 2 - Amendment 6

Supplement 6 to the 01 series of amendments — Date of entry into force: 24 September 2023

Uniform provisions concerning the approval of vehicles with regard to the location and identification of hand controls, tell-tales and indicators

This document is meant purely as documentation tool. The authentic and legal binding texts is: ECE/TRANS/WP.29/2023/21.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Paragraph 5.3.3.,* amend to read:

"5.3.3. The indicators, their identifications and the identifications of controls need not be illuminated when at least one of the following conditions apply:

1. the headlamps are being used to give intermittent luminous warnings at short intervals;
2. the headlamps are operated as daytime running lamps;
3. daytime running lamps are switched on."

1. \* Former titles of the Agreement:

   Agreement concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

   Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)