|  |  |
| --- | --- |
|  | E/ECE/324/Rev.2/Add.124/Rev.3/Amend.2−E/ECE/TRANS/505/Rev.2/Add.124/Rev.3/Amend.2 |
|  |  | 20 June 2023 |

 Agreement

 Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

(Revision 3, including the amendments which entered into force on 14 September 2017)

\_\_\_\_\_\_\_\_\_

 Addendum 124 – UN Regulation No. 125

Revision 3 - Amendment 2

Supplement 2 to the 02 series of amendments – Date of entry into force: 5 June 2023

 Uniform provisions concerning the approval of motor vehicles with regard to the forward field of vision of the motor vehicle driver

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2022/122.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

 *Paragraph 1.1.,* amend to read:

"1.1. This UN Regulation applies to the 180° forward field of vision of drivers of category M1 and N1 vehicles.[[2]](#footnote-3)"

 *Paragraph 1.3.,* amend to read:

"1.3. The requirements of this UN Regulation are so worded as to apply to category M1 and N1 vehicles in which the driver is on the left. In category M1 and N1 vehicles in which the driver is on the right these requirements shall be applied by inverting the criteria, when appropriate."

1. \* Former titles of the Agreement:

 Agreement concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

 Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)
2. As defined in the Consolidated Resolution on the Construction of Vehicles (R.E.3.), document ECE/TRANS/WP.29/78/Rev.6, para. 2. – https://unece.org/transport/vehicle-regulations/wp29/resolutions [↑](#footnote-ref-3)