|  |  |  |
| --- | --- | --- |
|  | **INF.18** | |
| **Economic and Social Council**  Inland Transport Committee  **Working Party on the Transport of Dangerous Goods**  **Joint Meeting of Experts on the Regulations annexed to the  European Agreement concerning the International Carriage  of Dangerous Goods by Inland Waterways (ADN) (ADN Safety Committee)**  **Forty-third session**  Geneva, 22-26 January 2024  Item 5 (b) of the provisional agenda  **Proposals for amendments to the Regulations annexed to ADN:**  **other proposals** | | 17 January 2024  Original: English |

Proposal for using an easy-to-read table in 7.1.5.0.2 of ADN

Use of blue cones vessels carrying the dangerous goods listed in in Table A of Chapter 3.2 in packages placed exclusively in containers.

Submitted by the European Barge Union and the European Skippers Organization (EBU/ESO).

|  |
| --- |
| *Summary* |
| **Related documents**: Informal document INF.8 of the forty-second session  Informal document INF.17 of the forty-second session  Report of the forty-second session (ECE/TRANS/WP.15/AC.2/86 (Paragraph 63))  ECE/TRANS/WP.15/AC.2/2024/9 |
|  |

Introduction

1. The Government of France transmitted a proposal for an amendment to 7.1.5.0.2 of the Annexed Regulations to ADN, by means of working document ECE/TRANS/WP.15/AC.2/2024/9 for the forty-third session.

2. EBU/ESO is very pleased with the wording of the proposal.

3. Nevertheless, EBU/ESO would like to propose using a table instead of the proposed text.

4. This table has the same content and context of the proposed text, but is easier to read, easier to understand and easier to apply than the text displaying the legal content.

Proposal

5. Use text and table below in ADN instead of text:

"7.1.5.0.2 Vessels carrying the dangerous goods listed in Table A of Chapter 3.2 in packages placed exclusively in containers are not required to display the number of blue cones or blue lights indicated in column (12) of Table A of Chapter 3.2, unless otherwise indicated in the following table:

|  |  |  |  |
| --- | --- | --- | --- |
| **Number of cones/lights indicated in table A column (12):** | **Class and packing group of the substance:** | **Total gross mass:** | **Number of cones/lights to be displayed:** |
| **1 cone/light** | **Class 2 or PG I** | **> 130.000 kg** | **1 cone** |
| **Class 2 or PG I** | ≤ **130.000 kg** | **0 cones** |
| **Other classes or PG II or III** | **All masses** | **0 cones** |
| **2 cones/lights** | **Class 2 or PG I** | **> 30.000 kg** | **2 cones** |
| **Class 2 or PG I** | ≤ **30.000 kg** | **0 cones** |
| **Other classes or PG II or III** | **All masses** | **0 cones** |
| **3 cones/ lights** | **All classes** | **All masses** | **3 cones** |

"